SpeedFan 4.37
Copyright 2000-2008 by Alfredo Milani-Comparetti (alfredo@almico.com)

You can find SpeedFan at:

http://www.almico.com

What it does:
SpeedFan is a freeware program that monitors fan speeds and temperatures in computers with
a known monitoring chip. Its main feature is that it can control the speed of the fans
according to the temperatures inside your pc, thus reducing noise and power consumption.
SpeedFan can also access S.M.A.R.T. data and temperatures from EIDE, SATA and SCSI hard
disks.

How to setup:
Use the installer and read the HELP FILE.

Feedback:
Feel free to contact me at alfredo@almico.com if you've got any question or suggestion or
discover any strange behaviour.
I would like to receive an e-mail from those of you who try and find useful my program.
Not much: just a line of text.
Thanx for your attention :-)

History:
4.37 - fixed a bug where, after resuming from suspend, fan speeds were not really
       changed
     - added full support for AMD CD5536 SMBus
     - added identification of Fintek F75111R
     - fixed an Exotics tab Access Violation
     - fixed a bug that caused all of the EVENTS to be lost after entering CONFIGURE
4.36 - greatly improved temperature reporting for almost all nVidia video cards
     - now fan speeds are lowered more aggressively
     - added support for AMD K11 temperature sensor
     - added full support for SMSC EMC6W201
     - added full support for SMSC SCH5127
     - added support for SMSC EMC2710P fan speed readings
     - ARECA RAID support updated to Build 270
     - added AMCC/3ware test code
     - improved IT8720F identification
     - fixed F1 context sensitive help key support
     - better identification of DIRECT RAMBUS modules
     - enabled Intel ICH8 SMBus, if needed
     - identified SMSC SCH5317
     - some addresses on the Asus P5N32-E SLI are no longer scanned
     - some addresses on the Asus Rampage Formula are no longer scanned
     - some addresses on EVGA NFORCE 680i LT SLI are no longer scanned
4.35 - released to the public the EXOTICS tab
     - fixed 120 DPI issue in CONFIGURE dialog
     - added full support for Areca RAID controllers
     - greatly improved SCSI support
     - added support for Abit uGuru 3 (uGuru 2005)
     - added full support for Intel FB-DIMM temperature readings
     - added full support for ITE IT8720F
     - added full support for Andigilog aSC7611
     - added full support for LM96000 (it was previously detected as LM85B)
     - added full support for Analog Devices ADT7490
     - added full support for SMSC SCH5327
     - fixed Windbond W83766HG hardware monitor detection on some Asus motherboards
     - improved CPU identification routines
     - added support for a new revision of the WINBOND W83637HF
     - added support for WINBOND W83637HF at unusual addresses
     - added support for Asus F8000 at unusual addresses
     - added identification of the SMSC SCH5514
     - added identification of SMSC EMC2300
     - added ITE IT8718F fifth fan speed reporting
     - added preliminary detection of the HECI driver
     - added identification of Analog Devices ADP3228
     - added identification of ITE IT8512F
     - added identification of Winbond W83667HG SuperIO chip
     - identified a new revision of Fintek F71872 hardware monitor subsystem
     - fixed a bug in SMSC LPC47M172 support code that prevented fan speeds to be
       properly reported
     - 45nm Intel CPUs with CPUID=0x10676 now use a Tjmax value of either 105C or 90C
     - added full support for nVidia MCP65 SMBus
     - added full support for nVidia MCP67 SMBus
     - added full support for nVidia MCP73 SMBus
     - added full support for nVidia MCP78S SMBus
     - added full support for VIA CX700M SMBus
     - added full support for Intel 82801JIB SMBus
     - fixed an issue where the Intel SMBus couldn't be accessed and messages like
       SMBus msg : SMB Error $14 : FAILED (50) were generated
     - enabled Intel ICH8M-E SMBus device, if needed
     - enabled 631xESB SMBus, if needed
     - enabled Intel 6300ESB SMBus if needed
     - enabled SMBus on Intel ICH9R, if needed
     - preliminary detection of AMD CD5536 SMBus
     - some SMBus addresses on Asus Striker Extreme are no longer scanned
     - SMBus is no longer scanned at address $2E on DELL XPS710
     - Tyan S2927 second SMBus is no longer scanned
     - some addresses on the SMBus of Asus P5NT WS are no longer scanned
     - some addresses on the SMBus of the Intel DX38BT are no longer scanned
     - some SMBus addresses are no longer scanned on Asus M2N32-SLI DELUXE
     - the second nForce SMBus is no longer scanned on FIC AU31
     - some addresses on the SMBus of Supermicro H8DCE are no longer scanned
     - added some SMBus scan exclusions for Intel D5400XS
     - added /NOGIVEIO command line parameter to disable access to giveio.sys
     - added /NOGEFORCEROM command line switch that will prevent SpeedFan from reading
       nVidia GeForce ROMs (useful if it takes too much time)
     - nVidia video BIOS is now stored in a file for later retrieval
     - fixed an access violation under Win9x with some nVidia video cards
     - battery status messages are no longer displayed
     - upon resume, all controlled fans are set to 100% for half a second, then set to
       their minimum fan speed
     - added new configuration option SHOWSTATICICON
4.34 - added full support for SiS964 SMBus
     - added full support for SiS966 SMBus
     - added full support for ULi M1575 SMBus
     - added full support for VIA VT8237S SMBus
     - added full support for VIA VT8251 SMBus
     - added full support for nVidia MCP61 SMBus
     - added full support to read internal temperatures on AMD K10 processors
     - added native nVidia video card (up to, but excluding 8xxx) internal temperature
       reporting
     - added full support for SMSC SCH5307
     - added full support for F8000 temperatures and fan speeds
     - added full support for SMSC EMCT03
     - added full support for WINBOND W83793G, including ADVANCED options
     - added support for Fintek F71782F hardware monitor at unusual addresses
     - added support for Winbond W83627DHG at unusual addresses
     - added support for ITE IT8726F hardware monitor at unusual addresses
     - added support for a new stepping of the Andigilog aSC7621
     - Winbond W83791D now properly handles higher fan divisors for fan1, fan2 and fan3
       and shows fan4 and fan5 too
     - added SMSC LPC47M192 FAN DIVISOR settings in CONFIGURE / ADVANCED
     - added full PWM support to SMSC LPC47B397, including settings in CONFIGURE /
       ADVANCED
     - CONFIGURE now allows to go as low as -60C when selecting the DESIRED and WARNING
       levels to let users of the "relative" Intel Core temperature reading properly
       configure SpeedFan
     - improved DDR2 memory module size detection
     - added preliminary DDR3 identification
     - new SpeedFan icon by Bengt Strom
     - fixed an issue where Intel Core temperatures on multi core systems reported the
       same temperature for all cores
     - improved Tjunction detection for Intel CORE temperatures (you might no longer
       need the temperature offset in CONFIGURE / ADVANCED)
     - fixed crash on several DFI motherboards
     - fixed the detection of older revisions of the ITE IT8705F
     - restored the correct clock speed after resume from hibernation
     - rewritten the logic of the usage of a synchronizer in the thread that reads CPU
       usage (this will fix the SpeedFan not exiting issue)
     - address $2E on DFI motherboards is no longer scanned if the motherboard model
       starts with LP; if you have one of these models and you know that there should be
       a valid chip at that address, send me a SEND REPORT (INFO tab) with some NOTES
     - fixed ADT7475 temperature readings when in offset 64 mode
     - fixed a bug when changing the type of data to be charted
     - mails sent by SpeedFan now properly separate headers and the body with a blank
       line
     - fixed an issue with SUN 2864 motherboard
4.33 - completely rewritten the detection and the identification strategy of ITE IT871xF
       chips (fan readings are now ok)
     - xAP support is now properly reenabled between sessions
     - fixed context sensitive help (F1 key) on Windows Vista
     - enabled, if needed, the SMBus on Intel ICH7 and ICH8-M
     - added several checks to CPU usage routines, fixing a nasty issue where an error
       window appeared once every second
     - added full support for ATI SB600 SMBus
     - added full support for Intel ICH9 SMBus
     - added full support for nVidia MCP55 SMBus
     - added sull support for ADT7475
     - added nVidia Control Panel access to read video card temperatures
     - supported the IT8716F and the IT8718F hardware monitor at unusual addresses
     - added some SMB scan exceptions for Compal 08A0
     - SMBus address $15 no longer scanned on AOpen i975Xa-YDG
     - fixed an issue that caused the DFI LP UT NF4 SLI-DR Venus to power off on program
       start
     - added support for Fintek F71872F voltage readings
     - IT8712F-J now uses two undocumented FAN DIVs
     - speeded up Asus M2N32-SLI DELUXE program startup
     - added detection of an unknown Fintek chip (to avoid false detection of other
       sensors at the same address)
     - W83627EHF and W83627DHG now properly show SMARTFAN III in CONFIGURE / ADVANCED
     - W83627EHF and W83627DHG can now change PWM TYPE from PWM to DC in CONFIGURE /
       ADVANCED
     - fixed FAN DIVISOR settings for Winbond W83791D
     - added PWM OUT BASE CLOCK selection for WINBOND W83627DHG, W83627EHF and W83627EHG
     - warning temperature can now be set as high as 125C in CONFIGURE
4.32 - added a digitally signed 64 bit driver (fully tested under Vista 64 bit)
     - added full support for INTEL CORE DUO internal temperature readings
     - added full support for Andigilog aSC7621
     - added full support for Fintek F71882F
     - added xAP support to publish temperatures and fan speeds
     - improved support for Fintek F71782F
     - improved support for IT8716F
     - renamed temperatures readings for MAX6640
     - improved compatibility with Intel D975XBX2
     - reduced AD7416 and AD7417 false detections
     - reduced MAX6650/6651 false detections
     - improved Intel SMBus routines
4.31 - added full support for W83627DHG
     - added full support for VIA VT8237A
4.30 - added detection and support for internal temperature sensors on
       multiprocessor AMD K8 (Sempron, Athlon 64 and Opterons) systems
     - added full support for ADM1026
     - added full support for SMSC SCH311x
     - added full support for MAX6640
     - added full support for INTEL 631xESB SMBus
     - added full support for ADT7473
     - added LPC47M534 fan support
     - ADT7473 and ADT7476 temperatures now properly handle offset 64 setting
     - fixed W83637HF PWM MODE 3 and PWM 3 ENABLE setting
     - fully verified DFI LP NF4 support
     - added a check to skip SCSI disks that return invalid LOG SENSE pages
       (usually are EIDE/SATA disks where the driver tries to emulate some SCSI
       specific calls)
     - added preliminary detection of NS PC8374L, NS PC87427 and WINBOND W83627DHG
     - added an additional check in LM80 detection to avoid some false positives
     - improved ICH7-M support
     - added /NOAMDK8SCAN command line switch
     - 100% fan speeds on program exit is no longer a default
4.29 - added support for hardware monitor at unusual addresses on W83627EHF
     - fixed multiple instance detection of video cards
     - hard disk temperature is recomputed in the IN-DEPTH ONLINE REPORT
     - added detection and support for new revisions of IT8712F
     - added detection for some Analog Devices chips
     - optimized chart repainting
     - events can now send EMAILs using the built-in multithreaded server
     - SEND MAIL for events sends an email containing all current readings
       (temperatures, fans, fan speeds, voltages and hard disk status)
     - implemented hysteresis in fan speeds control (this should greatly
       reduce fluctuations)
     - fixed "error loading event" message at startup
     - added full support for NVIDIA MCP04
     - added full support for Intel ICH8 SMBus
     - identified some new Winbond W83627 revisions
     - added full support for AMD K8 internal temperature sensor
4.28 - added HD ONLINE ANALYSIS tool
     - added centralized INTERNET configuration tab in CONFIG dialog
     - added support for NForce410
     - added support for new video cards
     - added Temperature Sensor Type, BJT Offset and Gain support for Fintek F75375S
       in CONFIGURE / ADVANCED (on Asus V9999 you might need to set BJT OFFSET from
       174 to 202)
     - SMART overall indicators are computed using a more advanced strategy
     - updated the help file
     - properly fixed byte swapped HDD model names
4.27 - added full support FINTEK F75387 support
     - added full support for PHILIPS SA56004X
     - added support for FINTEK F71872F
     - properly enabled ICH6 SMBus when needed
     - added full support for SiS965 SMBus
     - events now play BEEP through the speaker's driver at a lower level
     - added full support for ANALOG DEVICES ADT7476
     - fixed a bug in the installer that prevented installing under some circumstances
     - added support for nVidia GeForce 6800 NV48 and 6610 XL
     - DELL support was extended to ICH7 motherboard models
4.26 - greatly improved nVidia support (it should no longer go to high CPU
       usage and /NONVIDIAI2C should be no longer needed)
     - EVENTS now can access SMART HD attributes
     - fixed a memory leak in events' processing
     - added full support for ANALOG DEVICES ADT7468
     - added support for more nVidia video cards
     - added support for ABIT AX8
     - fixed FINTEK F75375S fan speed change (previously it didn't work)
     - UGURU support is no longer probed through WMI (this fixes an error
       message that appeared to some users)
     - verified to be working fine under Windows Vista
     - added PWM control settings for WINBOND W83637HF in CONFIGURE / ADVANCED
     - added advanced settings for the third fan of W83637HF
4.25 - added EVENTS handling
     - added full ICH7 support
     - added full LPC47M233 support
     - fixed fan speed readings for SMSC LPC47B27X, LPC47M10X, LPC47M13X,
       LPC47M14X, LPC47M192, LPC47M292 and LPC47M534
     - revisited DELL SMBIOS routines: added support for a wider range of
       INTEL chipsets and for more temperatures on the same system
     - added preliminary support for ALI1573 SMBus
     - added full support for WINBOND W83627EHG
     - REMOTE temperature reading for LM99 now properly adds 16C
     - added an additional check when testing UGURU support
4.24 - added uGuru support
     - enabled GET CONFIG button on the INFO tab (please, read the help file)
     - added support for ALi M1563 with M1681
     - enabled online GET CONFIG procedure to download user supplied
       configurations for individual motherboard models
     - fan names set up by sensor's initialization code are now properly
       reflected in the UI
     - better detection of ITE IT8702F
     - identified a new revision of ITE IT8705F
     - added debug code and improved NS PC87366 support
     - fixed russian and added danish translation
     - Winbond W83791D and W83791SD do share the same Device ID and are now
       always detected as a Winbond W83791D
     - properly closed the I/O support routines when entering suspend
4.23 - added full 64 bit support for AMD64 systems
     - added full support for ATI SB300 SMBus
     - added full support for FINTEK F75375S
     - added chinese translation
     - completely rewritten the installer to handle the new services
     - properly initialized PortIO object when running under Win9x
     - removed a test related to LPC47N252 that caused some systems to freeze
     - fixed W83627EHF fan speed readings
     - added full support for NATIONAL SEMICONDUCTOR LM99 and LM63
4.22 - fixed temperature reporting for SCSI drives that do not fill all the
       relevant fields
     - added full support for FINTEK F75383 and F75384
     - added full support for FINTEK F75373S
     - fixed a misdetection of some IT8712F and IT8702F
     - added japanese translation and fixed hungarian one
     - identified a new version of WINBOND W83627HF
     - fully fixed and verified NATIONAL SEMICONDUCTOR LM85, ANALOG DEVICES
       ADM1027 and ADT7463 and SMSC EMC6D103 PWM speed settings
     - added advanced settings for MAXIM MAX6657 (some Asus or Samsung P35 users
       might find them useful)
     - fixed administrator privileges issue when installing
     - fully fixed WINBOND W83627EHF support for fan speed changing
     - fixed W83627EHF FANDIV4 and FANDIV5
4.21 - added full support for SCSI hard disks: besides SCSI hard disk temperature
       report, S.M.A.R.T. status is shown, including the full report for internal
       counters
     - added support for ATI SB400 SMBus
     - added full support for SMSC DME1737
     - added full support for GMT G768B
     - added full support for GMT G768D
     - AUTO FAN SPEED setting is no longer lost
     - fixed PWM3 MODE setting for Winbond W83627THF
     - added /NOSCSISCAN
     - fixed fan divisors for Winbond W83697HF
     - fixed an issue while probing ACPI temperatures
     - added indonesian (Henry Eko Hapsanto) and romanian (Vasilica-Mihai Horgot)
       translations
     - fixed LM90 local and remote readings (they were inverted)
     - properly identified a new revision of National Semiconductor LM85B
     - added preliminary support for National Semiconductor LM93
     - better handled RESUME FROM SUSPEND
4.20 - added support for a new revision of Analog Devices ADT7463
     - added full support for the SMBus in NForce4 chipset
     - properly identified a new version of Winbond W83627HF
     - added French (Skunnyk and Nicholas Aymeric), brazilian (Igor Andre) and
       slovak (Matus Lenhart) translations
     - added /NOACPISCAN command line switch
     - added ACPI temperature sensor
     - added PWM configuration options for Winbond W83697HF
     - added some code to avoid false LM80 detections
     - SmartGuardian setting is now left unchanged on ITE IT8712F
     - added PWMOUT CLOCK setting in CONFIG / ADVANCED for Analog Devices ADM1027
       and ADT7463, SMSC EMC6D103 and National Semiconductor LM85B and LM85C
     - added support for SMSC LPC47B397 temperatures and fan speeds
     - CLOCK settings are no longer lost
4.19 - fixed a bug in reading internal properties for some sensors
     - added ULi M1689 SMBus support
     - properly identified a different version of SMSC LPC47M172
     - improved IT8702F detection over the SMBus
     - trying to fully enable MANUAL PWM mode on SMSC EMC6D103
     - IT8712F support now may need you to enter CONFIG / ADVANCED to set the
       appropriate PWM MODE (please, read the help file)
     - fixed identification of S.M.A.R.T. and AAM for hard disks
     - added a new section in the help file to explain how to set Advanced Options
       for IT8712F and other chips (please read it if you no longer can change fan
       speeds)
     - added a new tip if an IT8712F is found
4.18 - added full support for NE1618
     - added manual multipliers (from 1 to 20) and divisors (from 1 to 20) for
       all fans (use CONFIG / ADVANCED)
     - added manual reverse for PWM logic in CONFIG / ADVANCED
     - SEND REPORT no longer accesses some NE1619 registers
     - added preliminary russian translation (thanks to Pavel Gourkov)
     - SiS741 SMBus is no longer identified as a SiS5595
     - added manual offsets for all temperatures (use CONFIG / ADVANCED)
     - added preliminary support LPC47M292
     - started using controls with a newer look
     - added preliminary Spanish and Galician translations
4.17 - added full support for WINBOND W83627EHF
     - added full support for INTEL 6300ESB
     - added several nForce2 motherboards to CLOCK tab's quick selection
     - properly identified NVIDIA GeForce FX Go 5600 and FX 5700
     - added a check to completely remove nVidia nForce2 SMBUs links that are
       actually unused
     - fixed the "You seem to have an NVIDIA graphic card." tip reappearing even
       if instructed not to do so
     - added support for new nVidia nForce2 chipset version
     - LM90 temperatures are now properly labeled LOCAL and REMOTE
     - added support for new revision of VT1211
     - fixed VT1211 hardware monitoring access
     - removed some PLEASE REPORTs
     - the ListView in the CHART TAB no longer sorts values when clicking on the
       header
     - fixed charting negative values
     - revised nForce2 CLOCK CONTROL internal routines improving overall stability
       and relialability
     - fixed representation of available CLOCK values for PLL20503
     - added full support for changing W83627HF and W83783S PWM OUT clock
       frequency
4.16 - verified support for nVidia nForce3 150 SMBus
     - added nVidia nForce2 clock control
     - identified nVidia GeForce FX Go 5200
     - added detection for LPC47m182
     - added detection for LPC47n350 new version
     - added detection for LPC47m976
     - added detection for LPC47m260
     - added support for W83627THF at non standard address
     - added special properties for ADM1031
     - fixed a mistake with ADM1031 properties
     - added detection for generic PC87591
     - added a link to SpeedFan's website on the INFO tab
4.15 - added full support for ICH6
     - added polish translation
     - added full support for ATI RADEON 9100 IGP (IXP150)
     - added support for a new version of ITE IT8712F
     - added czech translation (gvg [at] atlas.cz)
     - properly removed some sensors that are detected on two different BUSes
     - enabled SMBus on Intel ICH3-S, if needed
     - removed IDE IDENTITY dump from SEND REPORT
     - refined various translations
     - max temperature allowed in CONFIG is now 99C
     - fixed reading fan divisor for FAN2 on ADM1031
     - added full support for ADM1030
     - fixed "ERROR collecting CPU Usage" issue
     - new CPU detection routines (the "Exception in reading CPU INFO at startup"
       message should be gone)
     - detected more revisions of Winbond W83627THF
4.14 - fans are reset to 100% on exit even if using LOGOFF
     - added support for S.M.A.R.T. drivers that do not fully report requested data
     - charts properly show Fahrenheit, if needed
     - german translation
     - added full support for nVidia nForce 3 250
     - added full support for LM86
     - added full support for ADM1031
     - added support for W83792D
     - added support for Fujitsu-Siemens Hermes
     - added support for more nVidia Video Cards
     - now it can be selected whether pressing the X on the title bar causes
       SpeedFan to be minimized (EXIT from the icon menu always closes SpeedFan)
     - added support for the third PWM on W83627THF
4.13 - greatly improved nVidia Video Cards' I2C support
     - SEND REPORT no longer scans nVidia Video Cards
     - enabled NVIDIA video cards support after resume
     - added support for WORD READs to nVidia I2C, thus detecting available LM75
       sensors on that BUS
     - added support for GeForce Ti 4400
     - a bug tracking system is available at http://www.bugtrack.almico.com
     - added detection for LPC47M172
     - handled the inverse logic for PWM in LPC47M192
     - less debug messages are issued when problems are detected accessing the SMBus
     - made the LM75, AD7416, AD7417 temperature reading compatible with the higher
       resolution of the DS75
     - no longer probed for DDC monitors
     - removed WINBOND CLOCKS checking
     - GL525SM check is now done only at $2D
4.12 - added detection for PC87591
     - added new S.M.A.R.T. attributes
     - fixed calling help with F1 key no longer working due to a bug in Delphi 7
     - trying to avoid LM84 misdetection
     - trying to avoid MAX6650 misdetection
     - trying to avoid AD7417 misdetection
     - added full support for NE1619
     - better detection of AD7417
     - avoid duplicate detection of S.M.A.R.T. drives
     - trying to add fan control for DELL sensors
     - initialized disabled LM79
     - added full logging capability
     - added support for nVidia video cards
     - added full support for MAX6648
     - added detection for DDC monitors
4.11 - fixed the usual programming bug: a missing x:=x+1 in a while loop. I'm sorry,
       but all of the beta testers didn't trigger it :-)
     - added additional info to DEBUG.NFO file automatically generated by SpeedFan
       when started
4.10 - exiting the configuration dialog refreshes CHART names
     - better identified a false LM80
     - added full support for nForce3
     - added preliminary support for SERVERWORKS CSB5
     - added nForce2 cooling bits in CONFIGURATION / ADVANCED
     - added full support for ADM1027
     - new processors detected
     - added ability to read a PCI DEVICES database
     - trying to make PWM control work on more ASUS boards
     - added fourth temp for ASB100
     - added full support for ASUS MOZART-2
     - added preliminary support for PC87372
     - added full support for LM85C
     - added preliminary detection for LM63, LM64 and LM93
     - added full support for ADT7463
     - added full support for AMD8111 SMBus 1.0
     - fixed some LPC47M192 PWM readings
     - added support for IT8712F and IT8705F sensors at non standard address
     - added full support for EMC6D103
     - added preliminary detection for EMC6W201
     - added preliminary detection for EMCT03
4.09 - added full support for SIS655
     - added full support for ICH5
     - added full support for SIS746
     - added full support for W83627THF
     - added preliminary support for VT1211
     - added full support for VIA VT8237
     - reduced the amount of data output in the SEND REPORT for PCI devices
     - recognized more CPUs (mostly P3, Athlon and P4)
     - improved TYAN support
     - added support for ICS952005
     - values for some ITxxxx sensors are no longer restored when exiting (this should
       solve the "fans set to 100% upon program termination" issue on some MBs)
     - added support for ICS9248-171
     - changed fan and temp readings for VT8231
     - properly read large HDD size
     - added preliminary support for ICS 9248-39
     - added support for W311 (VIA EPIA M9000)
     - added automatic clock speed setting based on CPU usage
     - added preliminary support for FUJITSU SIEMENS (POSEIDON?)
     - tray icon shows last value and no longer the average
     - added preliminary support for EMC6D102
     - added preliminary support for ISC952607
     - added preliminary detection for ADT7316, ADT7317, ADT7318
     - added preliminary detection for ADT7516, ADT7517, ADT7518
     - added preliminary detection for ADT7460, ADT7461
     - added history charting
     - added support for alternate BLOCK operations with some INTEL ICHs
     - added detection for ICH slave address
     - extended the help file to describe new features
4.08 - added full support for nVidia nForce2 chipset
     - added full support for W83L785TS-S
     - added fan speed readings for ALi M1535D/D+
4.07 - enabled the brand new website!
     - added LM90 support
     - added EMC6D100
     - added TOSHIBA custom fan ON/OFF support
     - added full support for LM85C
     - added support for SMSC Hardware Monitoring Block
     - LPC47M15X and LPC49M192 can't be distinguished (according to what available
       datasheets say) and, therefore, all references to previous LPC47M15X detection
       have been converted to LPC47M192
     - fixed ADM1021 support (reported a READPWMSINTERNAL ERROR)
     - added W83L785R temperature sensor selection
     - added MAX6650 DAC Operating Mode ADVANCED CONFIGURATION
     - added support for ICS9250-37 (ASUS P4T and IWILL P4R533-N)
     - added support for W83L784R PWMs when set to MANUAL MODE
     - added EMC6D100 FAN ZONE/MODE and PWM CLOCK advanced configuration
     - added EMC6D100 PWM support
     - added LPC47M192 fan speed reporting
     - the installer now sets GIVEIO start type to AUTOMATIC for Windows NT4
     - added PWM CLOCK selection and PWM ENABLING (fan speed changing) for LPC47B27X
       LPC47M10X LPC47M13X LPC47M14X and LPC47M192
     - fixed TEMP2 reading on Myson MTP008
     - added some additional info in the report (ASCII)
     - added full support for SiS648
     - added full support for VT8235
     - avoiding misdetection of LM87
     - added PWM MODE and FAN DIVISOR selection in ADVANCED configuration for W83L784R
     - added new info in report about the HDD
     - added full support for MAX1668 and MAX1805
     - properly initialized IT8712/IT8705 PWM mode
     - added full support for SiS651
     - detected a new version of W83627HF
     - preliminary support for ADT7411
     - preliminary support for AD7416 and AD7417
     - preliminary detection for ADM1027
     - added full support for LM92
     - preliminary detection of VIA VT1211
     - added preliminary support for VT8231sensors
     - fixed IT8712F and IT8705F FAN3 DIVISOR configuration
4.06 - changed detection routine for MAX1617
     - properly detected and handled SiS961
     - completely rewritten the configuration file. This is a major update I've been
       working on for a long time. This new configuration file properly handles
       computers where hardware monitoring devices appear and disappear and/or are
       swapped out (like S.M.A.R.T. HDDs).
       You should consider deleting SPEEDFANSENS.CFG before running this new release.
     - refined the configuration file: now it stores advanced properties set in the
       configuration dialog (ADVANCED tab)
     - ADVANCED configuration supports IT8712F temperature sensors mode
     - ADVANCED configuration supports IT8693F, IT8702F and IT8712F fan divisors
     - added full support for W83637HF
     - slightly revisited S.M.A.R.T. window to better show info reported by HDs with
       a lot of attributes
     - S.M.A.R.T. attributes are now shown with an icon telling the status of
       individual relevant attributes (STOP below 10%, WARNING below 40% and OK
       otherwise). Other attributes are only informative and an icon has no reason to
       be :-)
     - added support for SIS645DX (the one on ASUS P4S533)
     - fixed MTP008 PWMs and voltages readings
     - added full support for SIS650
     - fixed hibernation support
     - added MAX6650 PWM support
     - properly handled reversed logic PWM used on IT8712F
     - added full support for ADM1032
     - added a button (INFO tab) to find SMBus devices: this might be useful to
       search for CLOCK chips and if I need to know more about your motherboard :-)
     - the results from FIND SMBUS DEVICES are added to the usual REPORT
     - changed the way INTEL 82801 SMBus access is enabled if the BIOS didn't do it
       for you
     - added full support for Intel ICH-4
     - added full support for ADM1028
     - verified MAX6657 detection
     - fixed MAX6650 fan speed readings
     - added full support for NVIDIA SMBus on nForce chipsets
     - enabled SMBus Block Operations for all SiS chipsets
     - added HOW TO SEND A REPORT help topic
     - SEND REPORT now asks for basic info on fan speed changing ability for your
       motherboard
     - updated the help file for S.M.A.R.T.
     - fixed a minor problem with the REMEMBER IT checkbox in the ADVANCED tab of the
       CONFIGURATION dialog
     - user selected properties for each sensor chip are properly restored after SUSPEND
     - updated the help file for the INFO tab
     - added preliminary support for W83L785R
     - finally managed to enable ADM1025 monitoring!
     - forced IT8693F starting monitoring, if needed
     - added preliminary ASUS VIDEO CARDs support under Win2K/XP (you need the latest
       version of SmartDoctor installed)
     - added an SMBUS DEBUG facility activated by using /SMBDEBUG command line switch
       (there is a full description of this feature in the help file)
     - WANTED and WARNING temperatures shown in CONFIGURATION dialog are now shown both
       in Celsius and in Fahrenheit
     - finally fixed MSI KT3 Ultra hanging while scanning SMBus
     - the installer should no longer abort if unable to change SERVICE startup mode
     - enabled accessing WINBOND chips located at unusual ISA addresses
     - trying to enable W83697HF if disabled
     - added preliminary detection for LM86
     - added preliminary detection for LM90
4.05 - added full support for SIS635, SIS645, SIS735, SIS740 and SIS745. This
       means, for example, that you can read values from your ASUS P4S333 :-)
     - added support for FSB changing. Currently there are only a few motheboards
       and PLLs that are supported. On my ABIT BP6, LUCKY STAR 6LX2 and ECS K7S5A
       it's working pretty fine :-)
     - WINBOND W83791SD is now properly detected, thus avoiding detection of
       unknown chips at the same address
     - those two buttons in the CONFIG dialog should now properly show even with
       large fonts
     - added context-sensitive help (available pressing F1) which includes the
       tutorial
     - the installer/uninstaller now removes every trace from both the HD and the
       registry
     - added some new code to better reset Intel SMBus
     - added some tips that can be disabled after their first appearance
     - added preliminary ADM1024 support (please, send reports)
4.04 - created full installer/uninstaller
     - completely removed DLPORTIO
     - the installer can remove the DLPORTIO service if it was previously installed
     - documentation has been moved to CHM format and so it no longer requires
       WORD :-)
     - properly detected W83L784R
     - preliminary detection for W83L785R
     - full support for MAX6657 and MAX6659
     - trying to avoid duplicated detection of the W83627HF on TYANs
     - fixed an error that caused the PERFORMANCE indicator for S.M.A.R.T. drives
       to return too high a value if nothing was wrong (this error is mostly
       cosmetic and nobody could see it, as it was rounded to 100% even if it was,
       internally, reporting 10000% :-))
     - added full support for ALi M1535D/D+ fan control
     - added support for FDC37N972
     - minor fixes to DELL support
     - removed the third FAN DIVISOR setting in ADVANCED CONFIGURATION for W83697HF
     - added full support for AMD768
     - fan speeds can now be changed by hand in the main window
     - fixed initialization of the ADM1025 on some motherboards
     - added full support for VIA8233A SMBus
     - added support for new revision of the AS99127F
     - moved INI to the registry so that restricted users can use it under NT/2K/XP
     - fixed W83L784R voltage readings
4.02 - new detection routine for WINBOND chips
     - fixed a bug in the CONFIGURATION dialog that prevented some users from
       accessing all available options when using large fonts on some video cards
     - by popular demand, I've added online a list of motherboards that are know
       to change fan speeds
     - restored and verified full support for W83697HF PWMs. I managed to figure
       out how to use them by walking through those million errors on the
       datasheet :-)
     - previous releases could issue a "WARNING : GIVEIO.SYS not started" without
       informing that the following second attempt actually succeeded. Now
       everything is more informative :-)
     - fixed a bug when too many temperatures are detected
     - added preliminary handling of specific sensors' options (you can find them,
       for a few Winbond sensor chips, in the configuration dialog under the
       ADVANCED tab)
     - added support for ALi M1535D+ from ALi Cyber ALADDiN
     - added support for DELL CPU temperature and for fan speeds, even if these
       readings are the result of some hacks and not the result of a public
       datasheet. Any info from DELL would be much appreciated. Anyway, please
       note that reported temperatures seem to be REALLY HIGH. I wouldn't play with
       fan speeds if not absolutely sure. But so many of you asked for DELL
       support, so... now you should have it :-)
     - configuration option named ENABLE DELL FANS has been changed to ENABLE DELL
       SUPPORT
     - added detection and full support for MC1066
     - S.M.A.R.T. temperatures are now read every minute
     - all readings are forcibly updated after any configuration change
     - fixed CPU USAGE under Win9x
     - added full support for ALi M5879
     - removed a false detection of an LPC47b37x that may happen sometimes when a
       W83627HF is actually there
     - added preliminary detection for LPC47M15X (PLEASE REPORT)
     - added preliminary detection for EMC6D100/EMC6D101 (PLEASE REPORT)
     - added two S.M.A.R.T. status indicators that show a summary of drive fitness
       and performance
     - added preliminary support for PC87360
     - added preliminary support for PC87363
     - added a new command line parameter (/TIGERMP) to add full support for TYAN
       TigerMP
     - fixed a bug when associating PWMs that could lead to a DEBUG message
     - added /NOTIMER command line parameter that will avoid SpeedFan from updating
       values. This option is useful to see if SpeedFan is able to properly detect
       your hardware and stop right after having done that
     - added /NOSMARTSCAN command line parameter. This option will force SpeedFan
       not to probe S.M.A.R.T. devices. This is useful if you're having problems at
       program startup right after HD probing. This has occurred a couple of times
       and the reason should be in a bad driver for the HD controller
     - fixed "PROCESSOR PERFORMANCE OBJECT NOT FOUND" error. Now it is trapped and
       a nice message is displayed. CPU usage won't be available, but everything
       else will be
     - decoded some additional info about DIMMs
     - added preliminary support for ServerWorks OSB4 (I need reports)
     - added preliminary support for WINBOND W83L784 (I need reports here, as
       datasheets, guess what?, are incomplete, missing or full of errors :-))
4.01 - the last PWM (SPEED) can be properly set once again (thank you Sander for
       making me notice it :-))
     - added an option to choose between CELSIUS and FAHRENHEIT when showing
       temperatures
4.00 - properly reported IT8712F voltages
     - SMBus support is enabled on some VIA686 revisions if disabled
     - added SiS5595 sensor support
     - properly reported IT8693F voltages
     - CPU USAGE is now shown on the main window and supports multiprocessor
       systems too
     - added CPU speed computation (it works only for processors after and
       including Pentium I, but it appears to be extremely precise :-))
     - minimum and maximum fan SPEED settings are now selectable in 1 increments
     - reported samples now show their measure units
     - the balloon hint now appears only when a different sensors set is detected
     - fixed initial reporting about IT8693F settings
     - added preliminary support for FDC37n972
     - added full support for SIS630 SMBus
     - added full support for SiS730 SMBus
     - the message "ISA seems to be unused" has been changed to type INFO,
       instead of WARNING because several of you were afraid about the message
       itself :-)
     - added support for PC87364 PWMs
     - added support for PC87366 PWMs
     - fixed detection and usage of VT8231 and VT8233 SMBus
     - slightly changed SEND REPORT when probing SMBus
     - on the main window, the EXIT button has been replaced by MINIMIZE
     - finally fixed and tested all voltage readings from GL518SM (now
       everything is in sync with the datasheet)
     - added support for S.M.A.R.T. drives that report temperatures
     - added a TAB with S.M.A.R.T. info
     - enabled temperature monitoring on PC87366 if in standby
     - enabled S.M.A.R.T. monitoring for those HDs that have got it disabled
     - completely rewritten tray icon support
     - tray icon background and text colors are now fully configurable
     - IT8705/IT8712 voltages' readings are now enabled if BIOS didn't
3.07 - I've completely rewritten the installation procedure.
       Actually, now, there is none :-)
       You should no longer need to put any needed file nowhere, as SpeedFan is
       able to recreate them on the fly :-)
     - DLPORTIO.SYS and DLPORTIO.DLL need not to be manually put anywhere as
       SpeedFan should be able to recreate them if missing
     - fixed a bug with label when disabling ALL fans or ALL temps or ALL voltages
       or ALL speeds; if you try to reproduce this bug, please remember to check
       the fans each temperature is supposed to use; please note that this is not
       a bug in my code, but a "feature" from the compiler :-)
     - fixed an exception when sending a report using WinXP
     - GIVEIO.SYS needs not to be manually put anywhere as SpeedFan should be able
       to recreate it if missing, to install it as a service (under NT, 2k, XP) if
       not yet done and to start it if stopped :-)
     - autoinstalled GIVEIO.SYS if needed
     - changed icons: I know I'm not good with graphics, but I hope you will
       appreciate the effort :-) By the way: drawing a fan with THOSE 16 colors is
       not that easy :-)
     - /SUPERIO command line parameter has been removed: now SuperIO detection
       starts by default (I've done several tests with no reported crash :-)). If
       you need to disable SuperIO detection, use the /NOSUPERIO parameter instead
     - startup SMBus detection is now much faster; it you realize that some of
       your sensors are not properly detected, please use the /SLOWDETECT command
       line parameter and let me know
     - current PWM values (speeds) are updated after RESUME
     - confirmed full support for variating fan speeds with SMSC LPC47M13X
     - added preliminary detection for a lot of new SMSC and NATIONAL SuperIO 
       chips
     - fixed MTP008 fan speed reporting
     - fixed an error with PWM readings from ADM1021
     - redesigned the REPORT PREVIEW dialog
     - the report sends info about the SMBus (I've created this test in order to
       be able to create a faster startup sensor detection; PLEASE SEND AS MANY
       REPORTS AS POSSIBLE)
     - ADM1025 properly initialized if not yet enabled
     - fixed ADM9240, DS1780 and LM81 initialization
     - fixed a problem when setting PWMs
     - reversed PWM max and min logic on IT8712F: the datasheet says nothing on
       this subject, so I had to guess :-)
     - ADM9240, DS1780 and LM81 are properly initialized if not yet enabled
     - minor debugging changes to INTEL and VIA SMBus routines
     - added preliminary detection for FMS2701 (PLEASE REPORT)
3.08 - restored the proper use of MUTEXes: this should fix the problems when
       running SF together with other hardware monitoring softwares. I don't know
       how it could happen, but the compiler put an "END." in the wrong place,
       thus removing my INITIALIZATION routine
     - W83601R now properly reports its revision
     - trying to detect IT8703F
     - added full support for ALi M1533 South Bridge
     - the report now includes an ISA scan
     - initial detection of SiS5595
     - fixed GL520SM TEMP2 and +12V readings
     - properly handled MODE 1 and MODE 2 readings from GL520SM
     - rewritten THMC50 detection (PLEASE REPORT)
     - slightly revised INTEL SMBus code
     - initial test to try to enable disabled SMBus Hosts on INTEL 82801BA (ICH2)
     - initial test to try to enable PMU on ALi south bridges where it's
       currently disabled
     - full support for INTEL 440MX SMBus
     - added detection for more SuperIO chips
     - added a progress dialog when sending the report
     - SIS5595 now should show the temperature reading (but it needs to be
       enabled by the BIOS)
     - trying to enable fan speed control for LPC47b27x
     - trying to access SIS5595 SMBus
     - greatly reduced the amount of debugging info shown on the main window
     - added full support for VIA VT8231 SMBus
     - added preliminary support for VIA8231 sensors
     - slightly modified the starting sequence for VIA SMBus access
     - added preliminary support for PWM with IT8693F
     - reinstalled GIVEIO service if previous installation got broken
     - added PC87366 voltage and temperature readings
     - added MAX1669 temperature reading
     - properly enabled SMBus support on Intel 82801 south bridges
     - added MAX1669 PWM (or DAC, depends on original settings) support
     - added full support for LPC47m10x fan speed reading and setting
     - trying to access LPC47N252 PWMs
     - preliminary MAX6650 fan speed reporting
     - added support for DELL NOTEBOOKS. If you can't variate fan speeds with
       the controls on the main window, you might try to check the DELL option
       in the configuration dialog. This is actually something that works on
       DELLs, but there is no official info on this subject. It is based on a
       research from Michael Henze. It has been successfully tested on Latitude
       CPi D266XT and Inspiron 8000. Please, let me know if it works on your DELL
     - better detection of problems when sending reports
     - GL518SM should be fixed at last! this chip drove me crazy, but I found a
       PC with it and, finally, understood what was causing the problem :-)
     - added preliminary MAX6655 detection (PLEASE REPORT)
     - revised VIA SMBus support
     - added full support for LPC47N252 PWMs (tested on a DELL INSPIRON 8000,
       even though it's not that useful as I was unable to find any temperature
       sensor...)
     - trying to enable PMU on ALi M1533, M1543 and M1535D/D+ if not yet enabled
     - WINBOND has informed me that W83697HF has got no PWM :-(
     - added support for PC87364 and PC87366 fan speed readings
3.06 - complete SMBus support for VIA VT8233 M2
 b1  - rewritten ALi1543 detection
     - revised ALi SMBus access
     - added support for SiS85C503 DAM Module FAN speed reading
     - added (beta) support for Intel 82801CAM (ICH3) (PLEASE REPORT)
     - added and fully tested ALi M1543 SMBus support (thank you Samuel!)
     - added +5VSB and VBAT readings to W83697HF
     - fixed -5V and -12V readings for W83697HF
     - fixed internal routines when accessing PCI registers at invalid offsets
     - added and fully tested ALi M1535D SMBus support (thank you Graziano!)
     - when set to start minimized to tray, SF minimizes before doing any hardware
       detection
     - slightly speeded up SMBus transactions on INTEL and ALi
     - fixed a RANGE CHECK ERROR
     - SMBus failed transactions are now retried when they first fail
     - written a DOC to illustrate how to configure SpeedFan :-)
     - I've been told (thank you Alfred!) that on "ASUS A7V266, rev 1.06, BIOS
       v1002" you need to set CPU THERMAL OPTION, in your BIOS, to SHUTDOWN in
       order for SpeedFan to be able to variate fan speeds. Let me know about your
       experience :-)
3.04 - changed the order of detection for some sensors
b8.5 - no longer displayed AS99127F -5V and -12V readings
     - fixed GL518SM and GL520SM detection
     - added full support for GL518SM
     - VIA686 sensor chip now reports a few more data in the REPORT
     - added a BALLOON HINT at program startup (you need at least Win2k or Me I
       think)
     - I hope the tray icon is ok now :-)
     - default minimum value for fan speeds is now set to 0%
     - fan speeds are no longer variated as a default (you must enable them); I
       had to set it this way because a lot of users reported they couldn't change
       fan speeds, but it was due to the fact that SF was restoring them to
       appropriate values (according to temperature readings)
     - if a sensor is detected on ISA and then found again on SMBus, that SMBus
       address is no longer probed for other sensors
     - tried to distinguish between VIA686A and VIA686B
     - LM80 detection is delayed if all others fail
     - added a CONFIG option to start SPEEDFAN minimized
     - fixed an occasional bug in VIA TEMPs' readings (RANGE CHECK ERROR)
     - VIA686 is handled properly on a Soltek SL-75KAV, thanx to Janko Laszlo :-)
     - this version should work fine on every motherboard with VIA686
     - fixed a minor bug with AS99127F that was introduced with an internal beta
       release :-)
     - rewritten decoding of WINBOND and ASUS chips; I hope they are all fine now
     - added support for the fourth PWM register available in Winbond's W83782D
     - added support for forced suspension (when no confirmation is asked to
       running programs)
     - SEND REPORT sends some additional info about which is your operating system
       and your CPU
     - beta test with a SOLTEK motherboard
     - all readings show a hint with their last, minimum, maximum and mean value
     - main window no longer shows double values (last and mean)
     - added register reporting for unknown WINBOND chips
     - added '/NOSMBSCAN' command line option to solve problems with those
       motherboards where SMBus contains some chips that hang the system when read
       from (like some SOLTEKs)
     - fixed a problem when too many sensors' reading were available (more than
       those that could be shown)
     - added full support for ADM1025
     - added fans' and pwms' readings for LPC47b27x
     - added '/SUPERIO' command line option to enable detection of LPC47xxxx
       SuperIO chips with integrated hardware monitoring capabilities
     - added preliminary detection for SMSC LPC47b27x
     - added preliminary support for LPC47B37x (PLEASE REPORT)
     - added preliminary support for LPC47M10X (PLEASE REPORT)
     - added preliminary support for LPC47M13X (PLEASE REPORT)
     - added preliminary support for LPC47M14X (PLEASE REPORT)
     - added preliminary support for LPC47S42X (PLEASE REPORT)
     - added preliminary detection for ADM1022 (PLEASE REPORT)
     - added preliminary detection for ADM1023 (PLEASE REPORT)
     - added preliminary detection for ADM1024 (PLEASE REPORT)
     - added preliminary detection for MAX6650 (PLEASE REPORT)
     - added preliminary detection for MAX6654 (PLEASE REPORT)
     - added preliminary detection for MAX1668 (PLEASE REPORT)
     - added preliminary detection for ADM1028 (PLEASE REPORT)
     - added preliminary detection for ADM1030 (PLEASE REPORT)
     - added preliminary detection for ADM1031 (PLEASE REPORT)
     - added preliminary detection for ADM1032 (PLEASE REPORT)
     - added full support for GL520SM
     - added preliminary detection for GL523SM (PLEASE REPORT)
     - trying to detect VIA686 sensors on SMBus
     - preliminary detection for SiS 85C503 (PLEASE REPORT)
     - trying to support AMD766 SouthBridge: PLEASE SEND ME SOME FEEDBACK as I do
       not have it at home and can't do any test by myself :-)
     - added preliminary IT8693F temperature and fan readings
     - trying to detect VIA VT8233
     - added a test in order to detect some ASUS hidden features
     - added detection for MYSON MTP008
     - added full support for MYSON MTP008
     - removed MINIMIZE button on the main window
     - added preliminary detection for NE1619 (PLEASE REPORT)
     - added a checkbox on the main window to enable or disable automatic fan
       speed variation in one easy step
3.02 - attempt to detect GL518SM (please REPORT if FOUND!)
     - attempt to detect GL520SM (please REPORT if FOUND!)
     - attempt to detect GL523SM (please REPORT if FOUND!)
     - attempt to detect MAX1618 (please REPORT if FOUND!)
     - attempt to detect MAX1619 (please REPORT if FOUND!)
     - attempt to detect MAX1669 (please REPORT if FOUND!)
     - attempt to detect THMC50 (please REPORT if FOUND!)
     - hibernate and suspend support verified ok
     - added W83782D voltages' readings
     - added preliminary W83781D voltages' readings
     - added W83783S voltages' readings
     - added W83627HF voltages' readings
     - added AS99127F voltages' readings
     - added full support for LM87
     - added a safety feature when auto-assigning used sensor in case the primary
       sensor that has been detected hasn't got temps or fans or pwms and the next
       one has some
     - used a different font for the trayicon
     - the trayicon now limits its values from -99 to 99 and properly shows negative
       values
     - added full support for LM78
     - added preliminary LM79 voltages' readings
     - sent additional debug info (telling me how sensors are shown on the main
       window)
     - added full support for LM84 (I hope so :-))
     - sent additional debug info (regarding some interesting internal registers for
       selected chips)
     - shown VOLTAGES
     - added full support for PWMs for IT8712F
     - IT8712F is set in PWM SOFTWARE MODE upon detection, but original settings are
       restored on program exit
     - fixed PROXY SETTINGS when sending a report (it couldn't be edited)
     - added full support for LM80
     - attempt to detect W83697HF
     - added preliminary W83697HF temps' readings
     - added preliminary W83697HF fans' readings
     - added preliminary W83697HF voltages' readings
     - added preliminary W83697HF pwms' support (the datasheet is far from bein
       clear on this subject, please REPORT!)
     - added detection for IT8702F
     - added preliminary IT8702F fans' readings
     - added preliminary IT8702F pwms' support
     - added preliminary IT8693F detection (please REPORT!)
     - -12V and -5V are not (yet) shown for AS99127F as there seem to be different
       ways to decode them and I need testing (send REPORTs, please :-))
     - if SpeedFan is started with '/NOPCISCAN' then no PCI scanning is performed
     - added preliminary support for DS1780, ADM9240 and LM81
     - restored standard titlebar icons :-)
     - added PRELIMINARY VIA686 voltages' readings (I need reports)
3.00 - completely rewritten the whole program :-)
 PR2 - tray icon background should be fixed now
     - added detection for multiple southbridges on the same PC
     - added detection for multiple sensors
     - sensors' selection and use is now fully configurable
     - added full support for ADM1021, THMC10 and MAX1617A
     - added detection for GL525SM
     - reenabled VIA VT82C596(B) support: it works perfectly now (it didn't work
       because I followed a datasheet in order to properly detect SMBus functionalities,
       but there was an error on the datasheet itself :-))
     - added support for Winbond W83781D with CHIPID=$11
     - added detection for VIA686 sensors
     - added VIA686 temperature sensors readings
     - added detection and support for MAX1617
     - added detection and support for ASUS AS97127F
     - added detection for LM84
     - added support for LM76, but I can't find any easy way to distinguish it from
       LM75. If you know you have an LM76 chip, I would be pleased to do some
       testing :-)
     - automatically preferred ISA access for sensors that are available on both ISA
       and SMBus
     - added VIA686 fan speeds readings
     - fixed a bug inside internal statistical computations
     - added icons to show temperatures' trend
     - completely rewritten configuration dialog
     - added support for LM78 and LM79 (needs test)
     - removed APPEARANCE tab
     - removed EXTRA tab
     - added preliminary SUSPEND support
     - automatically avoided reading from chips from which the user didn't select any
       value to be monitored
2.05 - applied changes to INTEL SMBus support to increase its compatibility with ICH,
       ICH0 and ICH2
     - DIMM INFO memo box is now READ ONLY :-)
     - FANx% are now properly disabled according to sensor capabilities
     - trying to ignore spurious high values for fan readings
     - fan readings are now reduced to one third as they are only informational and
       not vital, thus reducing BUS overhead
     - almost completely rewritten INTEL SMBus support
     - enabled support for Intel ICH2 SouthBridge (I wrote "AB" instead of "BA" in the
       code)... all CUSL2 users should be happy now :-) thanx to Massimiliano Battaglia
       for extensive testing and debugging!
     - added an option to specify your motherboard model when sending a report (please,
       use this feature :-))
     - added a preliminary detection routine for LM75 and LM78
     - negative temperatures should be handled properly now
2.03 - VENDOR ID=$FFFF and CHIP ID=$FF are no longer shown as detected
     - fixed a minor bug that caused two sensors to seem to be detected when they have
       got the same CHIP ID (like some from ASUS and WINBOND) (thanx to Aaron Larson)
     - removed a lot of debug messages from SMBus (mostly 'reset' and 'NOT completed')
     - added a filter on collected values (for temperatures) in order to ignore single
       peak readings that are obviously wrong
     - added FAN2 control for AS99127F (thanx again to Carlo Adami)
     - by popular demand :-) info on the main page are now put in a memo and can be
       cutted&pasted :-)
     - when in debug mode, the main page shows which southbridge has been detected
     - VT82C596 southbridge has been removed from the supported list as it has been
       reported not to work properly :-(
     - added a button for sending a report without having to cut and paste :-) you are
       not forced to specify an email address, but it would be of use in case you
       expect some support
2.02 - done extensive testing with SMBus and PIIX4E
 b1  - buffered all UI values to lower CPU usage
     - extensive testing of the new fan speeds' changing strategy
     - DIMM INFO seem to work fine though I'm not sure if it will work with every DIMM
     - starting tests to use AS99127F ($31), W83781D and W83782D fan ON/OFF
     - trying to use register $59 to control FAN1 on AS99127F ChipID=$5CA3, ID=$31 and
       ChipID=$12C3, ID=$31
     - preliminary AS99127F fan speed changing support thanx to Carlo Adami!
     - should have been fixed an overflow that led to showing -256MB with 256MB DIMMs
     - removed SCAN PCI FOR CHIPSET checkbox as it was a safety measure in case
       something didn't work properly with it, but nobody ever reported any problem
2.00 - added SUPERBETA DIMM readings to check SMBus functionality
 b5  - added AMD756 SMBus support
     - AMD756 support starts working!
     - buffered some UI values to lower CPU usage and improve reliability
     - Winbond sensors' detection routine shows ChipId and VendId for unknown sensors
     - DIMM info now shows a message if no info is found
     - tested with INTEL 82801AA
     - completely rewritten the logic that changes fan speeds
2.00 - added a checkbox to enable DEBUG MODE that will issue more info in the message
 b2    box
     - added PCI SCANNING to enable CHIPSET detection
     - added preliminary SMBus support for Intel PIIX4 and Intel PIIX4E
     - increased compatibility with other monitoring software
     - preliminary AMD756 detection
     - preliminary INTEL ICH 82801AA/AB/BA detection
     - preliminary VIA VT82C686A support
     - preliminary VIA VT82C596 support
     - completely rewritten sensor detection routines
     - avoided a FLOATING POINT ERROR
     - tested with Intel PIIX4tested with VIA VT82C686
     - tested with Winbond W83783S
     - added USE ISA BUS and USE SMBus options
1.00 - fan speed readings can be limited by a user defined value useful when bad values
       are retrieved from sensors)
     - added a user definable value for the delta value used to increase or lower fan
       speeds (useful for those of you with CPUs that change their temperature very
       quickly)
0.96 - if it's impossible to find SYS and DLL files in the EXE directory, then they're
       searched in default directories
     - Gudjon Adalsteinsson submitted a bug in processing WARNING TEMPERATURES when the
       temperature index was different from fan index: now it's fixed
0.95 - improved taskbar font appearance
     - taskbar icon is update only when necessary
     - taskbar appearance is now stored in INI
     - added option to set fans at full speed on program exit
     - SYS and DLL are now searched in the executable directory
0.94 - DLL and SYS files are searched in the same directory as the EXE (in earlier
       releases they were searched in a fixed path, causing some users to be unable
       to run the program properly)
     - used an internal font to show temperature 1 on the taskbar
     - added support for WINBOND W83627HF
0.92 - added basic taskbar icon showing temperature 1
     - buffered taskbar icons to speed up repainting
     - set to 100 the upper limit for fan speeds
0.90 - first public release
