/ ****
MODEL: ZH-A1

1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 3072    32 * 1536
                48 * 1024
         Color: 16 * 1536    32 * 768
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Supports serial communication mode
8. Supports serial program upgrade
9. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-A4

1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 4096     32 * 2048
                48 * 1360     64 * 1024
         Color: 16 * 2048     32 * 1024
                48 * 680      64 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Supports serial communication mode
8. Supports serial program upgrade
9. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-Un

1. Maximum Points: 10240 (color area halved)
    Monochrome: 16 * 640    32 * 320
         Color: 16 * 320    32 * 160
2. Support for all scanning
3. Support 4 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Um

1. Maximum Points: 16384 (color area halved)
    Monochrome: 16 * 1024    32 * 512
         Color: 16 * 512     32 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Uc

1. Maximum Points: 24576 (color area halved)
    Monochrome: 16 * 1536    32 * 768
                48 * 512
         Color: 16 * 768     32 * 384
                48 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-U0

1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 2048    32 * 1024
         Color: 16 * 1024    32 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U1

1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 3072    32 * 1536
                48 * 1024
         Color: 16 * 1536    32 * 768
                48 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-UF

1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 2048    32 * 1024
                48 * 680     64 * 512
         Color: 16 * 1024    32 * 512
                48 * 336     64 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U2

1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 4096    32 * 2048
                48 * 1360    64 * 1024
         Color: 16 * 2048    32 * 1024
                48 * 680     64 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U3

1. Maximum Points: 65536 (color area halved)
    Monochrome:  16 * 4096    32 * 2048
                 48 * 1360    64 * 1024
                 80 * 816     96 * 680
                128 * 512
         Color:  16 * 2048    32 * 1024
                 48 * 680     64 * 512
                 80 * 408     96 * 336
                128 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
         PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U4

1. Maximum Points: 102400 (color area halved)
    Monochrome:  16 * 4096    32 * 3200
                 48 * 2128    64 * 1600
                 80 * 1280    96 * 1064
                128 * 800
         Color:  16 * 3200    32 * 1600
                 48 * 1064    64 * 800
                 80 * 640     96 * 528
                128 * 400
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-U5

1. Maximum Points: 163,840 (color height halved)
    Monochrome:  16 * 4096     32 * 4096     48 * 3008     64 * 2560
                 80 * 2048     96 * 1704    128 * 1280    144 * 1136
                160 * 1024    176 * 928     192 * 848     208 * 784
                224 * 728     240 * 680     256 * 640
         Color:  16 * 4096     32 * 2048     48 * 1696     64 * 1280
                 80 * 1024     96 * 848     128 * 640
  Note: 12 interface with 8 rows high 08 interface with 4 rows high

2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
Model: ZH-U6

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                144 * 3640    160 * 3272    176 * 2976    192 * 2728
                208 * 2520    224 * 2336    240 * 2184    256 * 2048
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                144 * 1816    160 * 1632    176 * 1488    192 * 1360
                208 * 1256    224 * 1168    240 * 1088    256 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
Model: ZH-U7

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                160 * 3272    192 * 2728    224 * 2336    256 * 2048
                288 * 1816    320 * 1632    352 * 1488    384 * 1360
                416 * 1256    448 * 1168    480 * 1088    512 * 1024
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                160 * 1632    192 * 1360    224 * 1168    256 * 1024
                288 * 904     320 * 816     352 * 744     384 * 680
                416 * 624     448 * 584     480 * 544     512 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
Model: ZH-U8

1. Maximum Points: 1048576 (color area halved)
    Monochrome:  32 * 8192     64 * 8192     96 * 8192    128 * 8192
                160 * 6552    192 * 5456    208 * 5040    224 * 4680
                240 * 4368    256 * 4096    288 * 3640    320 * 3272
                352 * 2976    384 * 2728    416 * 2520    448 * 2336
                480 * 2184    512 * 2048
         Color:  32 * 8192     64 * 8192     96 * 5456    128 * 4096
                160 * 3272    192 * 2728    224 * 2336    256 * 2048
                288 * 1816    320 * 1632    352 * 1488    384 * 1360
                416 * 1256    448 * 1168    480 * 1088    512 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E1

1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 3072    32 * 1536
                48 * 1024
         Color: 16 * 1536    32 * 768
                48 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E3

1. Maximum Points: 65536 (color area halved)
    Monochrome:  16 * 4096    32 * 2048
                 48 * 1360    64 * 1024
                 80 * 816     96 * 680
                128 * 512
         Color:  16 * 2048    32 * 1024
                 48 * 680     64 * 512
                 80 * 408     96 * 336
                128 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E5

1. Maximum Points: 163,840 (color height halved)
    Monochrome:  16 * 4096     32 * 4096     48 * 3008     64 * 2560
                 80 * 2048     96 * 1704    128 * 1280    144 * 1136
                160 * 1024    176 * 928     192 * 848     208 * 784
                224 * 728     240 * 680     256 * 640
         Color:  16 * 4096     32 * 2048     48 * 1696     64 * 1280
                 80 * 1024     96 * 848     128 * 640
  Note: 12 interface with 8 rows high 08 interface with 4 rows high
     
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E6

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                144 * 3640    160 * 3272    176 * 2976    192 * 2728
                208 * 2520    224 * 2336    240 * 2184    256 * 2048
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                144 * 1816    160 * 1632    176 * 1488    192 * 1360
                208 * 1256    224 * 1168    240 * 1088    256 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E7

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                160 * 3272    192 * 2728    224 * 2336    256 * 2048
                288 * 1816    320 * 1632    352 * 1488    384 * 1360
                416 * 1256    448 * 1168    480 * 1088    512 * 1024
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                160 * 1632    192 * 1360    224 * 1168    256 * 1024
                288 * 904     320 * 816     352 * 744     384 * 680
                416 * 624     448 * 584     480 * 544     512 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-E8

1. Maximum Points: 1048576 (color area halved)
    Monochrome:  32 * 8192     64 * 8192     96 * 8192    128 * 8192
                160 * 6552    192 * 5456    208 * 5040    224 * 4680
                240 * 4368    256 * 4096    288 * 3640    320 * 3272
                352 * 2976    384 * 2728    416 * 2520    448 * 2336
                480 * 2184    512 * 2048
         Color:  32 * 8192     64 * 8192     96 * 5456    128 * 4096
                160 * 3272    192 * 2728    224 * 2336    256 * 2048
                288 * 1816    320 * 1632    352 * 1488    384 * 1360
                416 * 1256    448 * 1168    480 * 1088    512 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support, Ethernet port and three serial communication mode
8. automatically obtain IP, IP settings without
9. Support single direct connection and LAN communications
10. The network interface is fully compatible direct line of communication and cross-line
11. RS-232 serial communication for direct line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-Gm

1. Maximum Points: 16384 (color area halved)
    Monochrome: 16 * 1024
         Color: 16 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G0

1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 2048    32 * 1024
         Color: 16 * 1024    32 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G2

1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 4096    32 * 2048
                48 * 1360    64 * 1024
         Color: 16 * 2048    32 * 1024
                48 * 680     64 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G3

1. Maximum Points: 65536 (color area halved)
    Monochrome:  16 * 4096    32 * 2048
                 48 * 1360    64 * 1024
                 80 * 816     96 * 680
                128 * 512
         Color:  16 * 2048    32 * 1024
                 48 * 680     64 * 512
                 80 * 408     96 * 336
                128 * 256
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5
/ ****
MODEL: ZH-G4

1. Maximum Points: 144,384 (color area halved)
    Monochrome: 16 * 4096    32 * 4096     48 * 3008    64 * 2560
                80 * 2048    96 * 1704    128 * 1280
         Color: 16 * 4096    32 * 2048     48 * 1696    64 * 1280
                80 * 1024    96 * 848     128 * 640
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support
11. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5

/ ****
Model: ZH-G7

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                160 * 3272    192 * 2728    224 * 2336    256 * 2048
                288 * 1816    320 * 1632    352 * 1488    384 * 1360
                416 * 1256    448 * 1168    480 * 1088    512 * 1024
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                160 * 1632    192 * 1360    224 * 1168    256 * 1024
                288 * 904     320 * 816     352 * 744     384 * 680
                416 * 624     448 * 584     480 * 544     512 * 512
2. Support 1 / 4,1 / 8,1 / 16 scan
3. Support free partition
4. Support magical run edge (full screen / partition)
5. Support the countdown, temperature
6. Communication Interface: GPRS RS-232 U disk
7. U disk storage format supports all FAT32 / NTFS / EXFAT
8. U disk support program upgrade
9. Timer switch support
10. Full screen test support


/ ****
MODEL: ZH-Wn

1. Maximum Points: 10240 (color area halved)
    Monochrome: 16 * 640    32 * 320
         Color: 16 * 320    32 * 160
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Wm

1. Maximum Points: 16384 (color area halved)
    Monochrome: 16 * 1024    32 * 512
         Color: 16 * 512     32 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W0

1. Maximum Points: 32768 (color area halved)
    Monochrome: 16 * 2048    32 * 1024
         Color: 16 * 1024    32 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W1

1. Maximum Points: 49152 (color area halved)
    Monochrome: 16 * 3072    32 * 1536
                48 * 1024
         Color: 16 * 1536    32 * 768
                48 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W2

1. Maximum Points: 65536 (color area halved)
    Monochrome: 16 * 4096    32 * 2048
                48 * 1360    64 * 1024
         Color: 16 * 2048    32 * 1024
                48 * 680     64 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W3

1. Maximum Points: 65536 (color area halved)
    Monochrome:  16 * 4096    32 * 2048
                 48 * 1360    64 * 1024
                 80 * 816     96 * 680
                128 * 512
         Color:  16 * 2048    32 * 1024
                 48 * 680     64 * 512
                 80 * 408     96 * 336
                128 * 256
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W4

1. Maximum Points: 102400 (color area halved)
    Monochrome:  16 * 4096    32 * 3200
                 48 * 2128    64 * 1600
                 80 * 1280    96 * 1064
                128 * 800
         Color:  16 * 3200    32 * 1600
                 48 * 1064    64 * 800
                 80 * 640     96 * 528
                128 * 400
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W5

1. Maximum Points: 163,840 (color height halved)
    Monochrome:  16 * 4096     32 * 4096     48 * 3008     64 * 2560
                 80 * 2048     96 * 1704    128 * 1280    144 * 1136
                160 * 1024    176 * 928     192 * 848     208 * 784
                224 * 728     240 * 680     256 * 640
         Color:  16 * 4096     32 * 2048     48 * 1696     64 * 1280
                 80 * 1024     96 * 848     128 * 640
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-W6

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                144 * 3640    160 * 3272    176 * 2976    192 * 2728
                208 * 2520    224 * 2336    240 * 2184    256 * 2048
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                144 * 1816    160 * 1632    176 * 1488    192 * 1360
                208 * 1256    224 * 1168    240 * 1088    256 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
Model: ZH-W7

1. Maximum Points: 524288 (color area halved)
    Monochrome:  32 * 4096     64 * 4096     96 * 4096    128 * 4096
                160 * 3272    192 * 2728    224 * 2336    256 * 2048
                288 * 1816    320 * 1632    352 * 1488    384 * 1360
                416 * 1256    448 * 1168    480 * 1088    512 * 1024
         Color:  32 * 4096     64 * 4096     96 * 2728    128 * 2048
                160 * 1632    192 * 1360    224 * 1168    256 * 1024
                288 * 904     320 * 816     352 * 744     384 * 680
                416 * 624     448 * 584     480 * 544     512 * 512
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support and WiFi dual mode of communication
8. U disk support and WiFi program upgrade
9. automatically obtain IP, IP settings without
10. Supports all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-Mm

1. Maximum Points: 5376
      Tricolor: 16 * 336
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. U disk support communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT

/ ****
MODEL: ZH-M2

1. Maximum Points: 21760
      Tricolor: 16 * 1360    32 * 672
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5

/ ****
MODEL: ZH-M4

1. Maximum Points: 33792
      Tricolor:  16 * 1360    32 * 1056
                 48 * 704     64 * 528
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5

/ ****
Model: ZH-M7

1. Maximum Points: 174080
      Tricolor:  32 * 1360     64 * 1360     96 * 1360    128 * 1360
                160 * 1088    192 * 896     224 * 768     256 * 672
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5

/ ****
MODEL: ZH-S1

1. Maximum Points: 49152
    Monochrome: 32 * 1536    48 * 1024
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5

/ ****
MODEL: ZH-S2

1. Maximum Points: 65536
    Monochrome: 32 * 2048    48 * 1360
                64 * 1024    80 * 800
                96 * 672
2. Support for all scanning
3. Support 16 free partition
4. Support for full screen and run side by side partitions run
5. Support full screen dynamic background and dynamic background by district
6. Support N kinds of cool text animation
7. Support U disk and dual serial communication mode
8. U disk support program upgrade
9. Support for all U disk storage format FAT32 / NTFS / EXFAT
10. RS-232 communication line is straight line
  Connection follows
        PC ---- Device
         2 ---- 2
         3 ---- 3
         5 ---- 5